|  |  |
| --- | --- |
|

|  |
| --- |
| Mavotrans - Oplossingen voor bouw en akoestiek |

  |
| **Checklist for periodic inspection of Mafi plate** |
| **Company:**……………………………………………………………..…………………………………..………… | **Project:**……………………………………………………………..…………………………………..………… |
| **Name of supervisor for Mafi use** ……………………………………………………………..…………………………………..………… | **Project part::**……………………………………………………………..…………………………………..………… |
|  |  |  |  |
| **Assembly checkpoints** | **Yes** | **No** | **Remark** |
| 1. Is the Mafi plate visually in order and is the threaded pin in two directions perpendicular to the plate?
 |  |  |  |
| 1. Before installing, turn the (rounded centre) nut to 200 Nm with a torque wrench to check. Never use power tools.
 |  |  |  |
| 1. Place the Mafi plate on the floor. Provide a flat surface. If not, fill in.
 |  |  |  |
| 1. Place the brace on the Mafi plate.
 |  |  |  |
| 1. Tighten the (rounded centre) nut with a torque wrench to100 Nm. This is a little more than hand holding.Never use power tools.
 |  |  |  |
| 1. With wind force 6 or higher: check the mounting once a week. Check whether the (rounded centre) nut is still firmly attached.
 |  |  |  |
| **Disassembly checkpoints** | **Yes** | **No** | **Remark** |
| 1. Loosen the (rounded centre) nut with a torque wrench and remove the brace.
 |  |  |  |
| 1. Remove the Mafi plate and make sure that the threaded pin does not collide with anything.
 |  |  |  |
| 1. Is the Mafi plate visually in order and is the threaded pin in two directions perpendicular to the plate?
 |  |  |  |
| *If in doubt, tighten the (rounded centre) nut with a torque wrench to* 200 *Nm. Never use power tools.* |
| 1. Place the Mafi plate carefully and in an orderly manner directly into the crate.
 |  |  |  |
| **Remarks/actions** | **Copy sent to** |
|  | 1. … |
| 2. …. |
| 3. …. |
| 4. …. |
| 5. … |
| **Inspection carried out by** |
| Name:  |
| Initials:  |
| Date:  |
|  |
| **Seen by executor(s)** |
| Name:  |
| Name:  |
| Name:  |